This operation instructs the EMS to turn off TCA reporting for a list of TPs.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when pmTPSelectList is empty or contains invalid data.
4. UNABLE_TO_COMPLY - Raised if the EMS is unable to disable TCA for the specified TPs (pmTPSelectList),
    i.e. no TPs were disabled.
5. NE_COMM_LOSS - Raised when communication to managed element is lost.
