The operation allows an NMS to specify a list of routes jointly with their provisioned administrative state. If all routes of the SNC are successfully locked, then the SNC state transits to PENDING. If the SNC state was PARTIAL or PENDING, and at least one route is successfully unlocked, then the SNC state may transits to ACTIVE.
See state change diagram of sncState.

Note: The relationship between Bundled SNC service and the SNC with Multiple Routes feature requires further study and is not applicable for v3.0.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when an EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when any input parameter is syntactically incorrect.
4. ENTITY_NOT_FOUND - Raised when at least one route identifiers reference an object that does not exist.
5. NE_COMM_LOSS - Raised when communication to managed element is lost and this prevents any change to the SNC.
