tmf854.v1 > LODDuration_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The LODDuration_T Simple Type
Refer to LODNumSwitches_T. Values are in seconds.
<ApplicableTo>For non-revertive switches. 1+1 trail protection,1:N trail protection,2-F MSSPRING, 4-F MSSPRING</ApplicableTo>
Simple Type LODDuration_T
LODDuration_T is derived from unsignedLong type. There are several restrictions on the value. The range of the value is [0..18446744073709551615]. The schema processor collapses value's whitespace. The number of fractional digits is less than or equals to 0.

XML
-<xsd:simpleType name="LODDuration_T"> -<xsd:annotation> -<xsd:documentation> Refer to LODNumSwitches_T. Values are in seconds. <ApplicableTo>For non-revertive switches. 1+1 trail protection,1:N trail protection,2-F MSSPRING, 4-F MSSPRING</ApplicableTo> </xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:unsignedLong"> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) unsignedLong

Used-By
Element (1) PGPParameters_T/LODDuration

Generated by WSDLdoc ©