Get names of the PTPs (no FTP subclasses) that contain one or more of the NMS-specified TP layer rates and that are capable of containing CTPs that can be connected at one or more of the NMS-specified connection layer rates. This operation considers the capability/flexibility of the PTPs, not their current states.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when tpLayerRateList or connectionLayerRateList contain undefined rates.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.
