Represents the type of threshold value.

Valid values are:
"Highest"
"High"
"Low"
"Lowest"

Changes in the attribute lead to an AVC notification.

Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No
