Discover the containing PTP and any containing CTP(s) of this CTP. Return the complete object information for the containing PTP or FTP and any containing CTP(s).

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to the ME is lost.
