Operation void clearPMData (CIS SequenceOf Structs::PMTPSelect pmTPSelectList = NA, CIS SequenceOf Structs::PMTPSelect failedTPSelectList = empty list), in Class PerformanceManager

Documentation
This operation instructs the EMS to clear (reset) the PM registers for a list of measurement points. Within the request for each measurement point, one may specify the granularity (15min, 24hr, NA) and location (nearEnd and/or farEnd and/or bidirectional) for the PM registers that are to be reset.
Clearing PM gauge minimum, maximum, and average registers means to reset them to the current measurement; for the actual gauge measurement, it has no effect. This is not considered a failure case.
Clearing PM registers is done on best-effort basis. If registers could not be completely cleared for a subset of cases in the pmTPSelectList, a list identifying this subset is returned.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS is unable to support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when pmTPSelectList is empty or contains invalid data.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
Managed element or the TPs specifed have to exist.
Postconditions
The specified Performance Monitoring registers are cleared and a list of registers that could not be cleared is returned.
Semantics

Arguments

pmTPSelectList
/* in */ This struct contains the relevant data for the clearPMData request. This must not be empty.
failedTPSelectList
/* out */ List of points for which PM registers were not completely cleared. An empty list indicates that the total request was successful.