The attribute contains the name of another TMD which is considered to contain this TMD.
The semantics of the containment is that the TMD to be created shall inherit the layered transmission parameters and additional TP information from the containing TMD.

Readable by NMS? No
Writeable by NMS? Yes
Invariant? Yes
