Operation void getSupportedPTPNames (CIS SequenceOf Name ptpNames), in Class Equipment

Documentation
This operation implements the 'supports' relationship (see equipment model) between equipment and PTPs for the NMS and returns the names of PTPs only.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS- Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

ptpNames
/* out */ The PTP object names implemented on the equipment.