Operation void getAllFixedSubnetworkConnectionNamesWithTP (Name tpName = NA, CIS SequenceOf Enums::LayerRate connectionRates = empty list, CIS SequenceOf Name sncNames = NA), in Class MultiLayerSubnetwork

Documentation
Get the set of the names of fixed Subnetwork Connection(s) that contain the NMS-specified TP, constrained by the specified connection rates.
A TP may be a PTP in which case a full list of fixed SNCs using any of its contained CTPs is required. A TP may be a CTP, in which case only fixed SNCs using that CTP or any of its contained CTPs are required.
Both end CTPs and intermediate CTPs at the same layer are considered. In all cases, only the names of the fixed SNCs that also match the specified connection rate filter are returned.
All legs of a broadcast system can be retrieved using this operation where the source TP of the broadcast system is used as input to the operation. The output will be the list of individual SNC names that make up the broadcast system.
This operation also works if a GTP is supplied rather than a CTP. In this case, the layerRate is set to LR_Not_Applicable. If the GTP is part of a cross connection, the EMS returns the set of bundled SNC names that use the provided GTP as either an end point or an interior point.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter is syntactically incorrect.
4. ENTITY_NOT_FOUND - Raised when tpName references an object that does not exist.
5. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
Identified TP has to exist.
Postconditions
No change in the system.
Semantics

Arguments

tpName
/* in */ The Termination Point name for which fixed Subnetwork Connections are requested.
It is also possible to provide a GTP. The NMS may provide a CTP that is associated with a GTP. In this case, the EMS returns the set of bundled SNC names that use the containing GTP as either an end point or an interior point.
connectionRates
/* in */ The connection rates that constrain the fixed Subnetwork Connections. If the list is empty, all fixed Subnetwork Connections (fulfilling the TP constrain) contained in the Subnetwork are returned.
sncNames
/* out */ The list of fixed Subnetwork Connection names containing the provided TP, constrained by the connection rates.