tmf854.v1 > CrossConnect_T > active
LOCATION: file:/xsd/networkResources/SubnetworkConnection.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The active Element
Indicates if the cross-connect is active in the ME.
Element CrossConnect_T/active : boolean [0 .. 1]
The active element can have "xsi:nil" as an attribute. The active element in XML instance can be substituted with other elements.

XML Instance
Indicates if the cross-connect is active in the ME. <active>xsd:boolean</active>

﻿

Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:element minOccurs="0" name="active" nillable="true" type="xsd:boolean"> -<xsd:annotation> <xsd:documentation> Indicates if the cross-connect is active in the ME. </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) boolean

Used-By

Generated by WSDLdoc ©