Operation void getAllCurrentPMData (CIS SequenceOf Structs::PMTPSelect pmTPSelectList = NA, CIS SequenceOf PMParameterName pmParameters = empty list, CIS SequenceOf PMData pmDataList = NA), in Class PerformanceManager

Documentation
This operation allows the NMS to request a filtered set (scoped by the input parameter pmParameters) current PM data for a list of TP measurement points.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does support only history/previous data.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when pmTPSelectList is empty or contains invalid data.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
Managed element or the TPs specifed have to exist.
Postconditions
No change in the system.
Semantics

Arguments

pmTPSelectList
/* in */ List of TP identifications.
pmParameters
/* in */ This parameter specifies which PM parameters within the scope of the pmTPSelectList shall be contained in the file. An empty list means to store all supported parameters. The returned parameters are best effort, i.e. among the parameters specified only the subset of supported parameters will be stored.
pmDataList
/* out */ List of PM data for 24h or 15min PM collection bin.