This operation inhibits (deactivates, or turns off) alarm reporting on this equipment holder.

Note: If alarm monitoring is disabled, then alarm reporting is disabled even if Alarm Severity Assignment Profile would allow it.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY -	Raised when alarm reporting can not be disabled.
4. NE_COMM_LOSS - Raised when communication to the managed element is lost.
