Operation void enablePMData (CIS SequenceOf Structs::PMTPSelect pmTPSelectList = NA, CIS SequenceOf Structs::PMTPSelect failedTPSelectList = empty list), in Class PerformanceManager

Documentation
This operation instructs the EMS to turn on PM data collection for a list of TPs.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised if pmTPSelectList is empty or contains invalid data.
3. CAPACITY_EXCEEDED - Raised when the maximum number of simultaneously enabled monitoring points is exceeded.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
Managed element or the TPs specifed have to exist.
Postconditions
All TPs specified for collection of Performance Monitoring Data are enabled and a list of non-supported subset is returned.
Semantics

Arguments

pmTPSelectList
/* in */ List of PM Selectors. Shall specify the name for an ME to select all TPs contained or shall specify a Termination Point list.
failedTPSelectList
/* out */ This is the list of TP names which could not be enabled.