tmf854.v1 > EQ_Inventory_T > supportedPTPNameList
LOCATION: file:/xsd/networkResources/Inventory.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The supportedPTPNameList Element
The PTPs that are returned are those that share their physical layer with the primary equipment (i.e. that represent a port on the equipment or are connected by a fibre, wire, etc.). The FTPs that are returned are those which are implemented by the physical circuitry supported by the equipment and will include FTPs that are named from the specified equipment (the FTPs will depend upon the presence of that equipment for their most basic operation). When there is equipment protection, this list reports PTPs/FTPs for the primary equipment only. That is, when called on a protecting equipment (as opposed to the primary equipment), this list returns an empty list, irrespective of the current switch status.
Element EQ_Inventory_T/supportedPTPNameList : NamingAttributesList_T [0 .. 1]
The supportedPTPNameList element cannot have "xsi:nil" as an attribute. The supportedPTPNameList element in XML instance can be substituted with other elements.

XML Instance
The PTPs that are returned are those that share their physical layer with the primary equipment (i.e. that represent a port on the equipment or are connected by a fibre, wire, etc.). The FTPs that are returned are those which are implemented by the physical circuitry supported by the equipment and will include FTPs that are named from the specified equipment (the FTPs will depend upon the presence of that equipment for their most basic operation). When there is equipment protection, this list reports PTPs/FTPs for the primary equipment only. That is, when called on a protecting equipment (as opposed to the primary equipment), this list returns an empty list, irrespective of the current switch status. <supportedPTPNameList extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T"> <name extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</name> [0..*] </supportedPTPNameList>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:element minOccurs="0" name="supportedPTPNameList" type="NamingAttributesList_T"> -<xsd:annotation> <xsd:documentation> The PTPs that are returned are those that share their physical layer with the primary equipment (i.e. that represent a port on the equipment or are connected by a fibre, wire, etc.). The FTPs that are returned are those which are implemented by the physical circuitry supported by the equipment and will include FTPs that are named from the specified equipment (the FTPs will depend upon the presence of that equipment for their most basic operation). When there is equipment protection, this list reports PTPs/FTPs for the primary equipment only. That is, when called on a protecting equipment (as opposed to the primary equipment), this list returns an empty list, irrespective of the current switch status. </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) NamingAttributesList_T

Used-By

Generated by WSDLdoc ©