The attribute contains additional info parameters which can be set and/or retrieved on an object having this TransmissionDescriptor (TMD) assigned as egress or ingress TMD.
Changes in the value of this attribute lead to an AVC notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
