tmf854.v1 > ConnectionDirection_T LOCATION: file:/xsd/networkResources/GlobalDefinitions.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The ConnectionDirection_T Simple Type
Direction of a subnetwork connection, cross-connects, or topological link. For a detailed description of the use of this attribute see SNC Types supporting document.
Simple Type ConnectionDirection_T
ConnectionDirection_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are

Enumeration | Description
CD_UNI | UNIdirectional, i.e. source TP to sink TP. Note: creation of unidirectional connections is supported even when CTPs/FTPs are modelled as bidirectional.
CD_BI | BIdirectional, i.e. bidirectional TP to bidirectional TP, a.k.a. two-way.

(CD_UNI | CD_BI).

XML
-<xsd:simpleType name="ConnectionDirection_T"> -<xsd:annotation> <xsd:documentation> Direction of a subnetwork connection, cross-connects, or topological link. For a detailed description of the use of this attribute see SNC Types supporting document. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> -<xsd:enumeration value="CD_UNI"> -<xsd:annotation> <xsd:documentation> UNIdirectional, i.e. source TP to sink TP. Note: creation of unidirectional connections is supported even when CTPs/FTPs are modelled as bidirectional. </xsd:documentation> </xsd:annotation> </xsd:enumeration> -<xsd:enumeration value="CD_BI"> -<xsd:annotation> <xsd:documentation> BIdirectional, i.e. bidirectional TP to bidirectional TP, a.k.a. two-way. </xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (3) CrossConnect_T/direction SubnetworkConnection_T/direction TopologicalLink_T/direction

Generated by WSDLdoc ©