This operation instructs the EMS to turn on PM data collection for a list of TPs.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised if pmTPSelectList is empty or contains invalid data.
3. CAPACITY_EXCEEDED - Raised when the maximum number of simultaneously enabled monitoring points is exceeded.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.
