LayerRate layerRate = NA, in Class SNCCreateData

Documentation
Identifies the layer at which the SNC is to be made.
Note: In case of creation of a bundled SNC the value LR_Not_Applicable has to be used. The EMS determines the layerRate(s) by looking at the CTPs contained in the aEnd and zEnd GTPs.
Readable by NMS? No
Writeable by NMS? Yes
Invariant? Yes

Export Control | PublicAccess | Containment | Unspecified
Static | No | Derived | No