Operation void enableTCA (CIS SequenceOf Structs::PMTPSelect pmTPSelectList = NA, CIS SequenceOf Structs::PMTPSelect failedTPSelectList = empty list), in Class PerformanceManager

Documentation
This operation instructs the EMS to turn on TCA reporting for a list of TPs.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when pmTPSelectList is empty or contains invalid data.
4. UNABLE_TO_COMPLY - Raised if the EMS is unable to enable TCA for the specified TPs (pmTPSelectList),
i.e. no TPs were enabled.
5. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
Managed element or the TPs specifed have to exist.
Postconditions
For those PM selectors which do not appear in the out parameter the TCA reporting is enabled.
Semantics

Arguments

pmTPSelectList
/* in */ List of PM Selectors where TCAs shall be enabled.
failedTPSelectList
/* out */ List of PM Selectors where TCAs could not be enabled.