Operation void disablePMData (CIS SequenceOf Structs::PMTPSelect pmTPSelectList = NA, CIS SequenceOf Structs::PMTPSelect failedTPSelectList = empty list), in Class PerformanceManager

Documentation
This operation instructs the EMS to turn off PM data collection for a list of TPs
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised if pmTPSelectList is empty or contains invalid data.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
Managed element or the TPs specifed have to exist.
Postconditions
The ME has stoped collection of Performance Monitoring Data as specified and gets an indication of the subset of TPs which can not be disabled.
Semantics

Arguments

pmTPSelectList
/* in */ PmTPSelectList. (see enablePMData() )
failedTPSelectList
/* out */ Out parameter: This is the list of TP names which could not be disabled.