This operation allows the NMS to request, from the EMS, the set of PM parameters supported by a particular ME at a specific layer.

Operation Exceptions:
1. NTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when neName does not reference a ManagedElement object or layerrate contains undefined rates.
3. ENTITY_NOT_FOUND - Raised when neName references an object which does not exist.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.
