tmf854.v1 > TPData_T > transmissionParams
LOCATION: file:/xsd/networkResources/SubnetworkConnection.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The transmissionParams Element
When used as output to the NMS, this is the transmission parameters of the TP. When used as input to the EMS, this is a "delta" list that needs to be applied to the specified TP. Only a subset of the parameters may be specified in the list, and only those should be applied in the NE. If the list is empty then this means do nothing. To remove a parameter from the list, "-" should be specified in the value part of the structure. When a BLSR connection is created, the SPRING_NodeId parameter should be provided for the aEnd and zEnd CTPs.
Element TPData_T/transmissionParams : LayeredParametersList_T [0 .. 1]
The transmissionParams element can have "xsi:nil" as an attribute. The transmissionParams element in XML instance can be substituted with other elements.

XML Instance
When used as output to the NMS, this is the transmission parameters of the TP. When used as input to the EMS, this is a "delta" list that needs to be applied to the specified TP. Only a subset of the parameters may be specified in the list, and only those should be applied in the NE. If the list is empty then this means do nothing. To remove a parameter from the list, "-" should be specified in the value part of the structure. When a BLSR connection is created, the SPRING_NodeId parameter should be provided for the aEnd and zEnd CTPs. <transmissionParams> <layeredParameters extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T">LayeredParameters_T</layeredParameters> [0..*] </transmissionParams>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:element minOccurs="0" name="transmissionParams" nillable="true" type="LayeredParametersList_T"> -<xsd:annotation> <xsd:documentation> When used as output to the NMS, this is the transmission parameters of the TP. When used as input to the EMS, this is a "delta" list that needs to be applied to the specified TP. Only a subset of the parameters may be specified in the list, and only those should be applied in the NE. If the list is empty then this means do nothing. To remove a parameter from the list, "-" should be specified in the value part of the structure. When a BLSR connection is created, the SPRING_NodeId parameter should be provided for the aEnd and zEnd CTPs. </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) LayeredParametersList_T

Used-By

Generated by WSDLdoc ©