CIS Boolean revertive = NA, in Class SubnetworkConnection

Documentation
The attribute defines if the SNC can be switched back to its original (intended) route.
In case the SNC is "revertive" (True), the restoration process will always switch to the intended route if possible, i.e. if there are no failures or if the intended route is not locked.
Changes in the value of this attribute lead to a AVC notification.
Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No