Operation void getActiveMaintenanceOperations (CIS SequenceOf Structs::CurrentMaintenceOperation_TP currentMaintenceOperationList = NA), in Class ManagedElement

Documentation
Retrieves all persistent maintenance commands that are currently enabled on this ME.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to the managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
All persistent maintenance commands that are currently enabled are retrieved.
Semantics

Arguments

currentMaintenceOperationList
/* out */ Includes all persistent maintenance commands that have been invoked for the given ME, for each TP, and layerRate if applicable.