Operation void setAlarmReportingOn (), in Class Equipment

Documentation
This operation allows (activates, or turns on) alarm reporting on an instance of the Equipment class. Only alarms from the equipment (not on TP alarms) are set on.
Note: If alarm monitoring is enabled, this does not mean that alarm is reported anyway, because Alarm Severity Assignment Profile may perform further filtering.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY - Raised when alarm reporting can not be enabled.
4. NE_COMM_LOSS - Raised when communication to the managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
Alarm monitoring is enabled on the specified equipment.
Semantics