This operation allows an NMS to request all of the pieces of equipment supported by the equipment, e.g., a power pack might support many circuit packs.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.
