This operation will return the SubnetworkConnections whose userLabel is supplied as a parameter.
This operation also works for bundled SNCs.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.
