CIS SequenceOf Structs::GuiCutThroughData guiCutThroughDataList = NA, in Class GCTProfileInfo

Documentation
The list of records associated with each supported window type and how to launch them. If the EMS does not provide data for a desired window type, the NMS may use an alternative data record such as the top level window. (The EMS top level window is the only window that is mandatory for the EMS to support.)
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No