Operation void getPotentialFixedCCs (Name containingTP = NA, CIS SequenceOf CrossConnect potentialCCList = empty list), in Class TerminationPoint

Documentation
The operation is used to retrieve fixed multiplexing and fixed inverse multiplexing schemes.
If the provided TP may be or is involved in a multiplexing or inverse multiplexing scheme, it will report:
1) the TP containing the fixed layer
2) the list of potential fixed cross connects that will exist if the containing TP's clientConnectivity or serverConnectivity is set to "Connected" (i.e. if the containing TP is currently multiplexing or inverse multiplexing).
If the clientConnectivity (resp. serverConnectivity) of the TP is currently set to "Connected", the potentialCCList matches the list of active fixed cross connects that are involved in its client TPs (resp. server TPs).
If the TP client layer (resp. server layer) is always fixed cross connected (hard-wired), the potentialCCList always matches the list of active fixed cross connects that are involved in the client TPs (resp. server TPs).
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY - Raised when TP is neither a higher order TP that supports fixed multiplexing
nor a lower order TP that supports fixed inverse multiplexing.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
TP is either a higher order TP that supports fixed multiplexing or a lower order TP that supports fixed inverse multiplexing.
Postconditions
No change in the system.
Semantics

Arguments

containingTP
/* out */ The TP supporting the attribute clientConnectivity or serverConnectivity.
potentialCCList
/* out */ Contains the list of all fixed cross connects of that multiplexing scheme, i.e. the list of cross connects that will exist when the containing TP clientConnectivity or serverConnectivity is set to "Connected". The A_end TPs of the cross connects should be the low order TPs that can be flexibly cross connected, and the Z_end TPs the TP clients of the high order TP. The list of cross connects does not have to be ordered.