This operation allows an NMS to request all the names of the equipments and equipment holders that are contained in the managed element.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.
