tmf854.v1 > EProtectionSwitch_T > neTime
LOCATION: file:/xsd/networkResources/Notifications.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The neTime Element
The time provided by the NE. In a case where the NE does not report time, this field is optional or an empty string can be reported.
Element EProtectionSwitch_T/neTime : ITU-Time_T [0 .. 1]
The neTime element cannot have "xsi:nil" as an attribute. The neTime element in XML instance can be substituted with other elements.

XML Instance
The time provided by the NE. In a case where the NE does not report time, this field is optional or an empty string can be reported. <neTime>ITU-Time_T</neTime>

﻿

Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:element minOccurs="0" name="neTime" type="ITU-Time_T"> -<xsd:annotation> <xsd:documentation> The time provided by the NE. In a case where the NE does not report time, this field is optional or an empty string can be reported. </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) ITU-Time_T

Used-By

Generated by WSDLdoc ©