Operation void getAllGroupTerminationPoints (CIS SequenceOf Enums::LayerRate layerRateList = empty list, CIS SequenceOf GroupTermminationPoint returnedGTPs = NA), in Class ManagedElement

Documentation
This operation allows an NMS to request all of the GTPs (on the ManagedElement) that contain one or more TPs at the specified layer rates.
If there are no GTPs that match the layer constraints, an empty list is returned.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when the layerRateList contains undefined rates.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

layerRateList
/* in */ Contains the list of layer rates for which the GTPs are to be fetched. A GTP must be associated to at least one CTP having one of the specified layer rates. If the list is empty then all GTPs (of all rates) are returned.
returnedGTPs
/* out */ Contains the list of GTPs that are accociated to CTPs of the specified layer rates.