Identifies a unidirectional measurement provided by a sink monitoring function that supervises the signal which is related to the sink atomic function of this TP. The direction of the supervised signal is measured.
See attached document for clarification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
