Operation void setAlarmReportingOn (), in Class SubnetworkConnection

Documentation
This operation activates alarm reporting on the subnetwork connection.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY - Raised when alarm reporting can not be enabled.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
Alarm reporting for the subnetwork connection is activated.
Semantics