tmf854.v1 > getTP_T LOCATION: file:/xsd/interfaces/ManagedElementMgr.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The getTP_T Complex Type
This service returns the termination point structure for the given TP name (CTP, FTP or PTP). The termination point name must be explicit (a generic endpoint specification may not be used in this case). See Object Naming for further detail on FTP naming. The termination point structure contains transmission parameters. The transmission parameters returned will be the parameters in place on the actual termination point on the NE. If there are no transmission parameters or the TP does not actually exist on the NE, then transmissionParams will be empty. The field transmissionParams will also be empty for "potential" ATM VP/VC CTPs. Raises ProcessingFailureException EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when tpName does not reference a termination point object EXCPT_ENTITY_NOT_FOUND - Raised when tpName references a TP object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost

Local elements (1)
  tpName

Complex Type getTP_T
The getTP_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T"> The retrieved TP name <tpName extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</tpName> [1..1] </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:complexType name="getTP_T"> -<xsd:annotation> <xsd:documentation> This service returns the termination point structure for the given TP name (CTP, FTP or PTP). The termination point name must be explicit (a generic endpoint specification may not be used in this case). See Object Naming for further detail on FTP naming. The termination point structure contains transmission parameters. The transmission parameters returned will be the parameters in place on the actual termination point on the NE. If there are no transmission parameters or the TP does not actually exist on the NE, then transmissionParams will be empty. The field transmissionParams will also be empty for "potential" ATM VP/VC CTPs. Raises ProcessingFailureException EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when tpName does not reference a termination point object EXCPT_ENTITY_NOT_FOUND - Raised when tpName references a TP object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost </xsd:documentation> </xsd:annotation> -<xsd:sequence> -<xsd:element name="tpName" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> The retrieved TP name </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> <xsd:attribute name="extVersion" type="xsd:string" use="optional" /> <xsd:attribute name="extAuthor" type="xsd:string" use="optional" /> <xsd:attribute name="tmf854Version" type="TMF854_Version_T" use="optional" /> </xsd:complexType>

﻿

Uses
Type (3) NamingAttributes_T string TMF854_Version_T

Used-By
Element (1) getTP

Generated by WSDLdoc ©