Indicates if the planned TP is to be configured such that it is capable of supporting lower rate connections (or is capable of supporting connections at the CTP's layer rate. 

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
