Specifies a list of PTPs, and/or CTPs that must be used by the route. The list must be empty if no PTP/CTP constraints are required. If the EMS cannot fully satisfy the constraints, then the request will be rejected.
