| **TS** | **CR** | **Rev** | **Rel** | **Title** | **Cat** | **Vsn** | **@ Mtg** | **TD#** | **Source to WG** | **Work Item** | **Clauses affected** | **Other Aff Specs** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 23.379 | 0223 | 1 | Rel-16 | Correct the error message is sent in the MCPTT emergency group call procedures | F | 16.3.0 | SA6#32 | S6-191418 | at&t | enh2MCPTT | 10.6.2.6, 10.6.2.6.1 |  |
| 23.379 | 0224 | 3 | Rel-16 | Correct the configuration parameters for the MCPTT emergency procedures | F | 16.3.0 | SA6#32 | S6-191588 | at&t | enh2MCPTT | A.3, A.3-1 |  |
| 23.379 | 0226 | 2 | Rel-17 | Call restrictions when using a specific functional alias for private calls | B | 16.3.0 | SA6#32 | S6-191556 | Nokia, Nokia Shanghai Bell | eMONASTERY2 | 10.15.3, A.3 |  |
| 23.379 | 0227 | 3 | Rel-16 | Corrections to MCPTT emergency alert procedures | F | 16.3.0 | SA6#32 | S6-191591 | at&t | enh2MCPTT | 10.6.2.6.3, 10.6.2.6.3.1, 10.6.2.6.3.3, 10.6.2.6.3.4 (new), 10.6.2.2.3b, 10.6.3.9.3.1, 10.6.3.9.3.2 |  |
| 23.379 | 0228 | 1 | Rel-16 | Add condition "not reachable" to call forwarding for MCPTT private calls | F | 16.3.0 | SA6#32 | S6-191446 | Kapsch CarrierCom | MONASTERY2 | 10.7.5.2.3 |  |