**3GPP TSG-SA WG6 Meeting #45-bis-e S6-212225**

**e-meeting, 11th – 19th October 2021 (revision of S6-21xxxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Clarification for Location reporting configuration | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | S6 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The description for MC service ID in table “10.9.2.1-1: Location reporting configuration” mentions “… MC service user **group** ….“ which should only be “… MC service user …” due to omitted change in implementation of CR0251r1. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Description for MC service ID in 10.9.2.1 is corrected. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Possible misinterpretation in the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 10.9.2.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* First Change \* \* \*

#### 10.9.2.1 Location reporting configuration

Table 10.9.2.1-1 describes the information flow from the location management server to the location management client for the location reporting configuration.

Table 10.9.2.1-1: Location reporting configuration

|  |  |  |
| --- | --- | --- |
| Information element | Status | Description |
| MC service ID | M | Identity of the MC service user to which the location reporting configuration is targeted. |
| Requested non-emergency location information | O  (see NOTE 1) | Identifies what location information is requested, except for emergency or imminent peril calls or emergency alerts |
| Requested emergency location information | O  (see NOTE 1) | Identifies what location information is requested, for emergency or imminent peril calls or emergency alerts |
| Triggering criteria in non- emergency cases | O  (see NOTE 1) | Identifies when the location management client will send the location report in non-emergency cases |
| Handling criteria in not reporting location information cases | O | Identifies when the location management client will store location information (e.g. never, off-network, IOPS) |
| Triggering criteria in not reporting location information cases | O  (see NOTE 2) | Identifies the causes when the location management client will generate location information |
| Minimum time between consecutive reports | O  (see NOTE 1) | Defaults to 0 if absent and 0 for emergency calls, imminent peril calls and emergency alerts |
| Triggering criteria in emergency cases | O  (see NOTE 1) | Identifies when the location management client will send the location report in emergency cases |
| NOTE 1: If none of the information elements is present, this represents a cancellation for location reporting based on Triggering criteria in emergency and non-emergency cases, if configured.  NOTE 2: If not present, location information is generated based on Triggering criteria in emergency and non-emergency cases, if configured. | | |

\* \* \* End Changes \* \* \*