**3GPP TSG-SA WG6 Meeting #49-e** **S6-221446**

**E-Meeting, 16th – 25th May 2022 (revision of S6-221031)**

Title: LS on TSN scenarios

Response to: -

Release: Release 17

Work Item: eSEAL

Source: SA6

To: SA2

Cc: -

**Contact Person:**

Name: Aron Szabo

E-mail Address: aron.szabo@ericsson.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

Attachments: None

# 1. Overall Description:

The implementation of the hold and forward function in DS-TTs is discussed in SA6. In this context, SA6 has the following question for SA2:

**Question:** Is UE-to-UE communication supported on the device side and no TSN data transfer on the N6 side for the TSN-integrated 5GS architecture, with the following clarifications to "System architecture view with 5GS appearing as TSN bridge” in Figure 4.4.8.2-1 of TS 23.501:

* Two communicating TSN end stations are on the device side instead of a single TSN station and these two TSN end stations communicate with each other.
* No TSN data transfer exists on the N6 / NW-TT side.

# 2. Actions:

**To SA2 group.**

**ACTION:** SA6 kindly requests SA2 to consider the above question.

# 3. Dates of Next SA6 Meetings:

3GPP TSG SA6#49-bis-e 06/2022 E-Meeting

3GPP TSG SA6#50 08/2022 Meeting (Wroclaw, PL)