**3GPP TSG-RAN WG3 Meeting #129 R3-255850**

**Bangalore, India, 25 – 29 August 2025**

Agenda Item: 19.2

Source: CATT, Ericsson

Title: (TP to TS 38.470 BL CR) Introduction of SBFD

Document for: Approval

# Introduction

This paper capture the following changes.

* Add abbreviation for CLI
* Add UE to UE CLI mitigation

# TP for BLCR to TS 38.470

3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

BH Backhaul

CLI Cross Link Interference

DRB Data Radio Bearers

eDRX extended Discontinuous Reception

eRedCap Enhanced Reduced Capability

F1-C F1 Control plane interface

<<<Unchanged part omitted>>>

5.2 F1-C functions

<<<Unchanged part omitted>>>

5.2. x CLI indication function

The CLI indication function enables the transfer of gNB-to-gNB CLI measurements, gNB-to-gNB CLI mitigation request and SRS Resource configuration between gNB-DU and gNB-CU.

<<<Next change>>>

## 6.1 Control plane procedures

<<<Unchanged part omitted>>>

6.1. x CLI indication procedure

The following procedure is used to report the result of gNB-to-gNB CLI measurements, to request mitigation of gNB-to-gNB CLI and request SRS Resource configuration:

- CLI INDICATION

<<<< End of change >>>