**3GPP TSG-SA5 Meeting #146Bis-e *S5-231097rev1***

**Electronic meeting, 16 - 19 January 2023**

**Source: MATRIXX Software**

**Title: pCR TR 32.847 Add new Key Issue on SBI between UE CHF and Tenant CHF**

**Document for: Approval**

**Agenda Item: 7.5.1**

# 1 Decision/action requested

**This pCR is to add a new Key Issue on SBI between UE CHF and Tenant CHF**

# 2 References

[1] 3GPP TR 32.847 "Study on Charging Aspects for Network Slicing Phase 2"

# 3 Rationale

This pCR is to add a new Key Issue on SBI between UE CHF and Tenant CHF.

# 4 Detailed proposal

The following changes are proposed to be incorporated into TR 32.847 [1]

|  |
| --- |
| **First change** |

## 6.x Key Issue #x: Service based interface between UE CCS and Tenant CCS

### 6.x.1 General Description

This Key Issue is for investigating on the selection for the service based interface between UE CCS and Tenant CCS to support solutions introduced with this distributed architecture under Key Issue #3, Key Issue #6 and Key Issue #7.

The investigation covers the following main capabilities for the service:

* Individual UE charging information from UE CCS to Tenant CCS: e.g. UE PDU session charging information in solution #3.1;
* UE CHF configured with indication on "dependency between UE charging and NS Charging": e.g. NS duration charging in solutions #7.2;

- NS Tenant Charging information exchanged between UE CHF and Tenant CHF in both directions: e.g. UE charging conditioned to NS charging information in solutions #6.1;This key issue relates to when standard interface between UE CCS and Tenant CCS is required.

|  |
| --- |
| **End of change** |