Documents for TSGN1 Ad-hoc meeting	Yellow cells indicate an allocated but not available Tdoc	
Agenda item	Agenda item title	Tdoc IW-99 	Title	Spec.	Source	Result	
1	Opening					22.11.1999 at 9:30 (estimate)	
2	Approval of agenda; document allocation	006	Agenda		Chairman	Noted. This file is a.k.a. Oulu9911.rtf	

							

3	Input Liaison statements						

							

							
4	GSM-UMTS related issues						
4.1	Impact of LLC removal on GMM 
New service primitives in MM/RAN IF			24.007			

4.2	2G MM / GMM evolution to 3G
New functional requirements on MM + GMM to make it MM + GMM + PMM			24.008
29.018			

							
							
4.3	Impact of LLC removal on SMS
New service primitives in SMS/MM IF			24.007			
							
4.4	Impact of LLC removal on SMS
Functional requirements on the SMS and MM protocols.			24.008
24.011
23.121			

							
							
4.5	MS CM changes			24.008			

							
							
4.6	Stage 2
Packet stage 2 is in 23.121 and 23.060.
Do we want to have some arrow diagrams in CS stage 2 also?			23.121
23.060

23.009			

							
							
4.7	Service continuity between 2G and 3G			24.008
what else ???			

							
							
4.8	Basic call handling changes			
23.003
23.009			

							
							
4.9	Indication of the optional and conditional items
There should be textual or other indication if a definition is limited to GSM only or UMTS only. This approach has already been taken by S2 in 23.060.			23.022
23.034 24.007 24.008 
27.001
etc.			

							
							
4.10	Suspend / Resume procedures
the procedures are needed for GSM R99. Are they needed for UMTS too or do they become conditional?			23.060
24.008			

							
							
4.11	Paging as CN message
GPRS GMM expects an indication of incoming paging to request for PAGING RESPONSE sending. The same principle will apply to UTRAN but are the service primitives the same?			23.060 24.008			

							
							
4.12	Ciphering
Indication of Ciphering key and algorithm(s) to mobile.			(23.108) 23.060 24.008			

							
							
4.13	Ciphering of initial MM message
No LLC -> no algorithm -> no ciphering for the initial PS GMM message.
S2 decision to add new message.			23.060 24.008			

							
							
4.14	Different subscriber identities
			23.060?
24.008		COMPLETE

IMSI will apply to both 2G and 3G,
no N1 action needed.
(S2-99633)	
							
4.15	New User Plane protocols, PDCP, BMC
TSGR#6 recently agreed on the introduction of PDCP and BMC.			24.007 24.008			

							
							
5 	Work Plan for TSGN WG1 for 1999					TSGN1 #8   25.-29.10.1999 (Japan/DoCoMo)
TSGN1 #9   30.11-3.12.1999 (Germany/Siemens)
TSGN #6 13.-15.12.1999 (Sophia Antipolis, France)
TSGN1 #10 11.-14.1.2000 (Japan/NEC)
SMG#31 14.-18.2.2000
TSGN1 #11 28.2.-2.3.2000 (Sweden/Telia)
TSGN#7  13.-15.3.2000
TSGN1 #12 22.-26.5.2000 (U.S./T1P1)
Please note that meeting #12 has been moved by one week to align with N3!!!
TSGN#8  19.-21.6.2000
SMG#32 26.-28.6.2000
TSGN1 #13 11.-15.9.2000 (U.S./T1P1)
TSGN#9  25.-27.9.2000
SMG#33 6.-10.11.2000
TSGN1 #14 27.11 – 1.12.2000 (Lucent)
TSGN#10 11.-13.12.2000	
		007	GSM-UMTS Interworking project plan		Chairman		

6	A.O.B.