{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Cover","SFN","Single tap","Multi-path fading"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #95-e",null,null,null,null,null,null,null,"R4-200xxxx"]
[null,"Electronic Meeting,  25 May - 5 June, 2020"]
[]
[null,"Source: Huawei, HiSilicon"]
[null,"Title: Summary of ideal and impairment results for NR HST demodulation requirements"]
[null,"Agenda: 6.17.2.1"]
[null,"Document for: Information"]

{"sheet":"SFN","index":1,"n_rows":6,"n_cols":24,"rows_kept":6,"cut":false,"hidden":false,"merged":[[2,0,5,0],[0,5,0,6],[0,9,0,10],[0,11,0,12],[0,13,0,14],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,15,0,16],[0,23,1,23],[0,19,0,20],[0,21,0,22],[0,7,0,8],[0,17,0,18]]}
["Propagation\ncondition","SCS\n[kHz]","CBW\n[MHz]","Maximum Doppler shift[Hz]","Antenna configuration","CMCC",null,"DOCOMO",null,"Ericsson",null,"Huawei",null,"Intel",null,"Qualcomm",null,"Vivo",null,"SPAN",null,"Average",null,"38.101-4 req"]
[null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["HST-SFN",15,10,870,"2x2",null,null,null,null,null,null,9.4,11.4,null,null,null,null,null,null,{"$f":"MAX(F3,H3,J3,L3,N3,P3,R3)-MIN(F3,H3,J3,L3,N3,P3,R3)","v":0},{"$f":"MAX(G3,I3,K3,M3,O3,Q3,S3)-MIN(G3,I3,K3,M3,O3,Q3,S3)","v":0},{"$f":"AVERAGE(F3,H3,J3,L3,N3,P3,R3)","v":9.4},{"$f":"AVERAGE(G3,I3,K3,M3,O3,Q3,S3)","v":11.4},{"$f":"W3+1","v":12.4}]
[null,15,10,870,"2x4",null,null,null,null,null,null,6.8,8.8000000000000007,null,null,null,null,null,null,{"$f":"MAX(F4,H4,J4,L4,N4,P4,R4)-MIN(F4,H4,J4,L4,N4,P4,R4)","v":0},{"$f":"MAX(G4,I4,K4,M4,O4,Q4,S4)-MIN(G4,I4,K4,M4,O4,Q4,S4)","v":0},{"$f":"AVERAGE(F4,H4,J4,L4,N4,P4,R4)","v":6.8},{"$f":"AVERAGE(G4,I4,K4,M4,O4,Q4,S4)","v":8.8000000000000007},{"$f":"W4+1","v":9.8000000000000007}]
[null,30,40,1667,"2x2",null,null,null,null,null,null,10.61,12.61,null,null,null,null,null,null,0,0,10.61,12.61,13.61]
[null,30,40,1667,"2x4",null,null,null,null,null,null,7.93,9.93,null,null,null,null,null,null,0,0,7.93,9.93,10.93]

{"sheet":"Single tap","index":2,"n_rows":8,"n_cols":24,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,19,0,20],[0,21,0,22],[0,23,1,23],[2,0,7,0],[0,7,0,8],[0,9,0,10],[0,11,0,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,0,6]]}
["Propagation\ncondition","SCS\n[kHz]","CBW\n[MHz]","Maximum Doppler shift[Hz]","Antenna configuration","CMCC",null,"DOCOMO",null,"Ericsson",null,"Huawei",null,"Intel",null,"Qualcomm",null,"Vivo",null,"SPAN",null,"Average",null,"38.101-4 req"]
[null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["HST single-tap",15,10,870,"1x2",null,null,null,null,6.41,7.41,7.87,9.870000000000001,null,null,null,null,null,null,{"$f":"MAX(F3,H3,J3,L3,N3,P3,R3)-MIN(F3,H3,J3,L3,N3,P3,R3)","v":1.46},{"$f":"MAX(G3,I3,K3,M3,O3,Q3,S3)-MIN(G3,I3,K3,M3,O3,Q3,S3)","v":2.4600000000000009},{"$f":"AVERAGE(F3,H3,J3,L3,N3,P3,R3)","v":7.1400000000000006},{"$f":"AVERAGE(G3,I3,K3,M3,O3,Q3,S3)","v":8.64},{"$f":"W3+0.8","v":9.4400000000000013}]
[null,15,10,870,"1x4",null,null,null,null,3.41,4.41,5.7,7.7,null,null,null,null,null,null,{"$f":"MAX(F4,H4,J4,L4,N4,P4,R4)-MIN(F4,H4,J4,L4,N4,P4,R4)","v":2.29},3.29,{"$f":"AVERAGE(F4,H4,J4,L4,N4,P4,R4)","v":4.5549999999999997},6.0549999999999997,{"$f":"W4+0.8","v":6.8549999999999995}]
[null,null,10,972,"1x2",null,null,null,null,6.41,7.41,7.91,9.91,null,null,null,null,null,null,1.5,2.5,7.16,8.66,9.4600000000000009]
[null,null,10,972,"1x4",null,null,null,null,3.42,4.42,5.68,7.68,null,null,null,null,null,null,2.2599999999999998,3.26,4.55,6.05,6.85]
[null,30,40,1667,"1x2",null,null,null,null,6.53,7.53,8.9700000000000006,10.97,null,null,null,null,null,null,2.4400000000000004,3.4400000000000004,7.75,9.25,10.050000000000001]
[null,30,40,1667,"1x4",null,null,null,null,3.53,4.53,7.46,9.4600000000000009,null,null,null,null,null,null,3.93,4.9300000000000006,5.4950000000000001,6.995000000000001,7.7950000000000008]

{"sheet":"Multi-path fading","index":3,"n_rows":9,"n_cols":24,"rows_kept":9,"cut":false,"hidden":false,"merged":[[0,19,0,20],[0,21,0,22],[0,23,1,23],[2,0,5,0],[0,7,0,8],[0,9,0,10],[0,11,0,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,0,6]]}
["Propagation\ncondition","SCS\n[kHz]","CBW\n[MHz]","Maximum Doppler shift[Hz]","Antenna configuration","CMCC",null,"DOCOMO",null,"Ericsson",null,"Huawei",null,"Intel",null,"Qualcomm",null,"Vivo",null,"SPAN",null,"Average",null,"38.101-4 req"]
[null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["HST multi-path fading",15,10,600,"2x2",null,null,null,null,6.22,7.22,6.7,8.6999999999999993,4.9000000000000004,6.9,6.68,8.68,null,null,{"$f":"MAX(F3,H3,J3,L3,N3,P3,R3)-MIN(F3,H3,J3,L3,N3,P3,R3)","v":1.7999999999999998},{"$f":"MAX(G3,I3,K3,M3,O3,Q3,S3)-MIN(G3,I3,K3,M3,O3,Q3,S3)","v":1.7999999999999989},{"$f":"AVERAGE(F3,H3,J3,L3,N3,P3,R3)","v":6.125},{"$f":"AVERAGE(G3,I3,K3,M3,O3,Q3,S3)","v":7.875},{"$f":"W3+0.5","v":8.375}]
[null,15,10,600,"2x4",null,null,null,null,2.7,3.7,2.94,4.9399999999999995,2.1,4.0999999999999996,3.07,5.07,null,null,{"$f":"MAX(F4,H4,J4,L4,N4,P4,R4)-MIN(F4,H4,J4,L4,N4,P4,R4)","v":0.96999999999999975},{"$f":"MAX(G4,I4,K4,M4,O4,Q4,S4)-MIN(G4,I4,K4,M4,O4,Q4,S4)","v":1.37},{"$f":"AVERAGE(F4,H4,J4,L4,N4,P4,R4)","v":2.7025000000000001},{"$f":"AVERAGE(G4,I4,K4,M4,O4,Q4,S4)","v":4.4525000000000006},{"$f":"W4+0.5","v":4.9525000000000006}]
[null,30,40,1200,"2x2",null,null,null,null,7.03,8.0299999999999994,7.6,9.6,7.2,9.1999999999999993,7.09,9.09,null,null,0.5699999999999994,{"$f":"MAX(G5,I5,K5,M5,O5,Q5,S5)-MIN(G5,I5,K5,M5,O5,Q5,S5)","v":1.5700000000000003},7.2299999999999995,{"$f":"AVERAGE(G5,I5,K5,M5,O5,Q5,S5)","v":8.98},9.48]
[null,30,40,1200,"2x4",null,null,null,null,3.5,4.5,3.54,5.54,3.8,5.8,3.39,5.3900000000000006,null,null,0.4099999999999997,{"$f":"MAX(G6,I6,K6,M6,O6,Q6,S6)-MIN(G6,I6,K6,M6,O6,Q6,S6)","v":1.2999999999999998},3.5575000000000001,{"$f":"AVERAGE(G6,I6,K6,M6,O6,Q6,S6)","v":5.3075000000000001},5.8075000000000001]
[]
[]
[null,null,null,null," "]