**3GPP TSG RAN WG2#111-e R2-20xxxxx**

**Online meeting, 17th - 28th August, 2020**

**Title: LS to SA2 on relay discovery assumptions**

**Response to:**

**Release:** Rel-17

**Work Item:** FS\_NR\_SL\_relay

**Source:** OPPO (to be RAN2)

**To:** SA WG2

**Cc:**

**Contact Person:**

**Name:** Zhongda Du

**E-mail Address:** [Du.Zhongda@oppo.com](mailto:Du.Zhongda@oppo.com)

**1. Overall Description:**

In RAN2#111-e meeting RAN2 agreed working assumption that Model A/B discovery model similar to LTE is reused for both UE-to-Network relay and UE-to-UE relay which is common for both Layer 2 based solution and Layer 3 based solution. During the discussion it is RAN2’s common understanding that final decision is up to SA2.

**2. Actions:**

RAN2 respectively ask SA2 to response your final decision for both UE-To-Network relay and UE-To-UE relay.

**4. Date of Next TSG-RAN WG2 Meetings:**

TSG-RAN WG2 Meeting #112e 2020-11-05 to 2020-11-16 E-Meeting