**3GPP TSG-RAN WG2 Meeting #114-e draft** R2-210xxxx

**Electronic meeting, 2021-05-19 – 2021-05-27**

**Title: draft** New LS on UE location aspects in NTN

**Response to:** -

**Release:** Release 17

**Work Item:** NR\_NTN\_solutions-Core, 5GSAT\_ARCH

**Source:** CATT [to be: RAN2]

**To:** RAN3, SA2, SA3, SA3-LI, CT1

**Cc:** -

**Contact Person:**

#### Name: Li Jianxiang

E-mail Address: lijianxiang@datangmobile.cn

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**1. Overall Description:**

As a follow-up information on top of what already indicated in the previous LS in R2-2102055 on UE location aspects in NTN, RAN2 would like to inform RAN3, SA2, SA3, SA3-LI and CT1 that RAN2 will be discussing a solution to ensure that the CGI constructed by NG-RAN corresponds to a fixed geographical area with a size comparable with a TN cell with a radius of ~2km for both connected mode and initial access.

Since the intention is to ensure this in connected mode and during initial access, this may be applicable also before AS security is activated.

RAN2 would like to ask SA3 whether a UE can report the location information with ~2km accuracy before AS security is established, e.g., during initial access.

**2. Actions:**

**To RAN WG3, SA WG2, SA WG3, SA WG3-LI and CT WG1**

**ACTION:** RAN2 kindly asks the above groups to take the above information into account, and provide any feedback if needed.

**3. Date of Next RAN2 Meetings:**

3GPP RAN2#115-e 16th – 27th August 2021 Electronic Meeting

3GPP RAN2#116-e 1st – 12th November 2021 Electronic Meeting