3GPP TSG-RAN WG2 Meeting #117-e  *R2-22xxxxx*

Electronic Meeting, 21 February – 3 March, 2022

**Title: [draft] Reply LS on Slice list and priority information for cell reselection**

**Response to: S2-2201859(R2-2203933)**

**Release: Release 17**

**Work Item: NR\_Slice-Core**

**Source: OPPO [to be RAN2]**

**To: SA2, CT1, RAN3, SA, RAN**

**Cc:**

**Contact person: Zhe, Fu**

fuzhe@OPPO.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** -

# 1 Overall description

RAN2 would like to thank SA2 for their reply LS on Slice list and priority information for cell reselection.

RAN2 has re-discussed the mapping of slice to the slice groups based on the latest SA2 LS.

A majority of companies in RAN2 expressed that the mapping of slice to the slice groups for cell reselection should be per TA. RAN2 understands the slice group granularity is an SA2 decision, However, RAN2 understands whether per TA or per PLMN granularity has no impact on RAN2 specification.

 RAN2 also assumes that the NAS layer in the UE is able to provide slice group priorities to AS layer in the UE.

RAN2 considers the WI is completed from RAN2 specification perspective based on the above assumptions. RAN2 requests other WGs to finalize their relevant specifications and indicate if RAN2 working assumptions are not valid before RAN#96.

RAN2 has achieved the following agreements.

1. A slice is not associated with multiple slice groups for the same purpose. A slice can be associated with one slice group for RACH and one slice group for reselection.
2. The UE AS is aware of the slice group ID (s) based on the information provided by the UE NAS.

# 2 Actions

**To SA2, CT1, RAN3, SA, RAN**

**ACTION:**

RAN2 kindly asks SA2, CT1, RAN3, SA and RAN to take the above information into consideration. Also, RAN2 expects SA2 to indicate if this RAN2 assumption does not work before RAN#96.

# 3 Dates of next TSG RAN WG2 Meetings

TSG-RAN2 Meeting #118-e May 16 – 27, 2022 Electronic Meeting