**3GPP TSG-RAN WG2 Meeting #129bis R2-2503168**

**Wuhan, China, 7 – 11 April, 2025**

**Title:** LS on AI/ML UE sided data collection

**Response to:** R2-2501759/S5-250828

**Release:** Rel-19

**Work Item:** AIML\_MGT\_Ph2

**Source:** RAN2

**To:** SA5

**Cc:** SA, SA2, SA3, RAN

**Contact Person:**

**Name:** Jun Chen

**E-mail Address:** jun.chen@huawei.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:**

**1. Overall Description:**

RAN2 would like to thank SA5 for their LS in R2-2501759/S5-250828 on AI/ML UE sided data collection.

For the SA5 assumption that the UP tunnel associated with data transfer is between UE and gNB for the solution 3, RAN2 has discussed the assumption and has made the following agreement:

* From RAN2 point of view UP tunnel between UE and gNB is not considered for 5GA R19/20, as currently the UP tunnel doesn’t terminate in the gNB

**2. Actions:**

**To SA5:**

RAN2 respectfully asks SA5 to take the above agreement into account.

**3. Date of Next TSG-RAN WG2 Meeting:**

TSG RAN2 Meeting #130 19 - 23 May 2025 Malta, EU

TSG RAN2 Meeting #131 25 - 29 Aug 2025 Bangalore, India