**3GPP TSG-SA3 Meeting #115 *S3-240912***

**Athens, Greece, 26 February -01 March 2024**

**Title:** LS on Issues related Analytics context transfer between AnLF(s)

**Response to:**

**Release:** Release 18

**Work Item:** eNA\_Ph3\_SEC

**Source:** 3GPP SA3

**To:** 3GPP SA2

**Cc:**

**Contact Person:**

#### Name: Rong Wu

E-mail Address: Raina.wu@huawei.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:**

**1. Overall Description:**

SA3 kindly ask SA2 to consider the following information.

SA3 noticed that in procedure of Transfer of analytics context and analytics subscription, as description in clause 6.1B of TS23.288, the Source AnLF may send the address (e.g. URL or FQDN) of Model file directly to the consumer(Target AnLF).

*Optionally, file address(es) of the trained ML model(s), which is included only when the source NWDAF itself provides the trained ML model(s) for the analytics subscription(s) for which the related analytics context is requested.*

The potential security issue is that the Source AnLF is not authorized by the NRF. The source AnLF could send the Model file address to the unauthorized AnLF. Regard this, SA3 suggests only Model ID(s) is allowed to be shared between AnLFs rather than model(s).

**2. Actions:**

**To SA2:**

**ACTION**: SA3 is kindly requested to take the above information into account.

**3. Date of Next TSG-SA WG3 Meetings:**

SA3#115-adhoc-e 15 Apr - 19 Apr 2024 TBD

SA3#116 20 - 24 May 2024 Korea, KR